
*Firmware update SunbriteTV*

**Step 1: Prepare the USB drive**

Unzip file onto an empty usb drive. Do not put the Zip file onto the usb flash drive; the update program is looking for MERGE.BIN.

This file needs to be copied to a USB flash drive that contains no other files or folders.

The filename must be named MERGE.BIN



**Step 2: Install the USB drive into the SunbriteTV Tuner board service port.**



**Step 3: Automatic update:**

Plug in the Usb drive containing the firmware update.

Unplug the AC power from the TV, wait 10 seconds, plug the AC power in. The board will read the USB drive and the front LED will start flashing.

Programming will take 2-3 minutes.

Do not interrupt the power or unplug the usb drive during the programming.

Once the programming is complete the LED will remain a steady red or blue.

Remove the USB drive and unplug AC power from the TV for 10 Seconds.

Plug in the AC power to the unit.


The setup may prompt for channel scanning, if you are not using the tuner, exit by pressing menu and select the desired input source.

**Step 4: Verify Firmware version**

**Press Source then 2-5-8-0**



The factory Menu should display. If the factory menu does not display press exit, then start over with Source then 2-5-8-0.



The software build time is the software version, in this case **July 17 2014, 11:02:55**